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Figure S1. Experimental setup of the beam collector (BC) and alternating-current current transformer (ACCT) under the linac treatment head at an extended source-to-surface distance (SSD) (pictured here, SSD = 32.3 cm). The beam arrives from the top, passing through a stack of collimators of decreasing diameter ending with the 4.5-cm collimator, which is directly atop the ACCT in all measurements. After the collimators, the beam passes through the 5.5-cm ACCT and finally impinges on the front surface of the BC. The ACCT is separated from the surface of the BC by two 2-mm-thick plastic blocks (light blue).
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